{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Arkusz2"],"not_rendered":{"macros":1,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Arkusz2","index":0,"n_rows":131,"n_cols":11,"rows_kept":131}
["l.p","Oznaczenie","Urządzenie","Krytyczność","Producent","TYP                                    Jedn.  zewn./ centrali","TYP                                 jedn.wewn. /nagrzewnicy","ROK PRODUKCJI","serwisów / rok","Cena ","Wartość"]
[1,"201-1.02-K","klimatyzator Split","nie","McQuay","M5LC015C-ACPOA-R","M5WM0156-ACIA",2010,2,null,{"$f":"I2*J2","v":0}]
[{"$f":"A2+1","v":2},"201-1.03-K","klimatyzator Split","nie","McQuay","M5LC015C-ACPOA-R","M5WM0156-ACIAC-R",2010,2,null,{"$f":"I3*J3","v":0}]
[3,"201-1.04-K","klimatyzator Split","nie","McQuay","M4LC015BAFCA","MWM015F-AFAH",2010,2,null,{"$f":"I4*J4","v":0}]
[4,"201-1.05-K","klimatyzator Split","nie","McQuay","M4LC015BAFCA","MWM015F-AFAH",2010,2,null,{"$f":"I5*J5","v":0}]
[5,"201-1.06-K","klimatyzator Split","nie","McQuay","M4LC010B AFCA","MWM010F-AFAH",2010,2,null,{"$f":"I6*J6","v":0}]
[6,"201-1.07-K","klimatyzator Split","nie","McQuay","M4LC010B AFCA","MWM010F-AFAH",2010,2,null,{"$f":"I7*J7","v":0}]
[7,"201-1.08-K","klimatyzator Split","nie","McQuay","M4LC020BAFCA","MWM010G-ACIAA-R",2010,2,null,{"$f":"I8*J8","v":0}]
[8,"201-1.09-K","klimatyzator Split","nie","McQuay","M4LC015BAFCA","M5WM0156-ACIAC-R",2010,2,null,{"$f":"I9*J9","v":0}]
[9,"201-1.10-K","klimatyzator Split","nie","McQuay","M4LC010B AFCA","MWM010G-ACIAA",2010,2,null,{"$f":"I10*J10","v":0}]
[10,"201-2.01-K","klimatyzator Split","nie","McQuay","M4LC010B AFCA","MWMOF-AFAH",2010,2,null,{"$f":"I11*J11","v":0}]
[11,"201-2.02-K","klimatyzator Split","TAK","McQuay","M4LC015BAFCA","MWM010G-ACIAA",2010,3,null,{"$f":"I12*J12","v":0}]
[12,"201-2.03-K","klimatyzator Split","nie","McQuay","M5LC020C-ACPOC-R","M5WM02oG-ACIAC-R",2010,2,null,{"$f":"I13*J13","v":0}]
[13,"203-1.11-K1","klimatyzator Split","TAK"," Samsung","AQ09FKX","AQ09FKN",2010,2,null,{"$f":"I14*J14","v":0}]
[14,"203-1.11-K2","klimatyzator Split","TAK","Kaisai","KWC-18CGO","KWC-18CGI",2022,2,null,{"$f":"I15*J15","v":0}]
[15,"203-1.11-K3","klimatyzator Split","TAK","Kaisai","KWC-18CGO","KWC-18CGI",2022,2,null,{"$f":"I16*J16","v":0}]
[16,"203-1.07-K","klimatyzator Split","nie"," Fujitsu","AQYR12LGC","AQ12FKN",2010,2,null,{"$f":"I17*J17","v":0}]
[17,"203-1.08-K",null,"nie"," Fujitsu",null,"ASYA12LACM",2010,2,null,{"$f":"I18*J18","v":0}]
[18,"203-1.10-K",null,"nie"," Fujitsu",null,"ASYA12GC",2010,2,null,{"$f":"I19*J19","v":0}]
[19,"203-1.12-K",null,"nie"," Fujitsu",null,"ASYA12LACM",2010,2,null,{"$f":"I20*J20","v":0}]
[20,"203-1.13-K","klimatyzator Multi Split","nie"," Fujitsu",null,"ASYA12LACM",2010,2,null,{"$f":"I21*J21","v":0}]
[21,"203-1.14-K","klimatyzator Split","nie"," Fujitsu","AOYA30LMAW4","ASYA12LACM",2010,2,null,{"$f":"I22*J22","v":0}]
[22,"203-2.7-K","klimatyzator Split",null,"AUX","AUX-09F2H/O","AUX-09F2H/I",2022,2,null,{"$f":"I23*J23","v":0}]
[23,"203-2.6-K","klimatyzator Split","nie","Kaisai","KWC-18CGO ","KWC-18CGI ",2022,2,null,{"$f":"I24*J24","v":0}]
[24,"204-KP1","klimatyzator przenośny ","nie","Superhobby Market",189684,null,2010,2,null,{"$f":"I25*J25","v":0}]
[25,"206-NG1","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-L-1700/300-3-1-P-T-1-(D-NW-ZW0",null,2010,2,null,{"$f":"I26*J26","v":0}]
[26,"206-NG2","linia grzewczo-nawiewna ","nie","VBW","SPS-2/50-P-3000/300-3-1-P-T-1-(D-NW-ZW)",null,2010,2,null,{"$f":"I27*J27","v":0}]
[27,"301-K1","klimatyzator Split","nie"," Fujitsu","AOYG18LAC2","ASYG09LJCA2",2011,3,null,{"$f":"I28*J28","v":0}]
[28,"301-K2","klimatyzator ścienny","nie",null,null,"AGYG09LV",2010,3,null,{"$f":"I29*J29","v":0}]
[29,"304-AWL1","Agregat wody lodowej","TAK","G.I. ITALY","CLINT CHA/K/SP153",null,2010,3,null,{"$f":"I30*J30","v":0}]
[30,"304-AWL2","Agregat wody lodowej","TAK","G.I. ITALY","CLINT CHA/K/363-P SI/PS/CT",null,2010,3,null,{"$f":"I31*J31","v":0}]
[31,"304-AWL3A","Agregat wody lodowej","TAK","LENOX","TSA030S4N4IT",null,2010,3,null,{"$f":"I32*J32","v":0}]
[32,"304-AWL4","Agregat wody lodowej","TAK","G.I. ITALY","CLINT CHA/K/SP91",null,2010,3,null,{"$f":"I33*J33","v":0}]
[33,"304-AWL5","Agregat wody lodowej","TAK","G.I. ITALY","CLINT CHA/K/SP151",null,2010,3,null,{"$f":"I34*J34","v":0}]
[34,"304-NNK1","klimatyzator Split","TAK","KAISAI","KGO-48NK3","KGD48K3F",2016,3,null,{"$f":"I35*J35","v":0}]
[35,"304-NNK2","klimatyzator Split","TAK","Hisense","AUW105U4RA4","AUW105U4RA4",2021,3,null,{"$f":"I36*J36","v":0}]
[36,"304-NW1","centrala klimatyzacyjna","TAK","VBW","BS-3(50)-L/P",null,2010,5,null,{"$f":"I37*J37","v":0}]
[37,"304-NW2","centrala klimatyzacyjna","TAK","VBW","BS-6(50)-L/P",null,2010,5,null,{"$f":"I38*J38","v":0}]
[38,"304-NW3","centrala klimatyzacyjna","TAK","VBW","BS-6(50)-L/P",null,2010,5,null,{"$f":"I39*J39","v":0}]
[39,"304-NW3A","centrala klimatyzacyjna","TAK","VTS","VENTUS VS-21-R-PHC",null,2010,5,null,{"$f":"I40*J40","v":0}]
[40,"304-NW4","centrala klimatyzacyjna","TAK","VBW","BS-6(50)-L/P",null,2010,5,null,{"$f":"I41*J41","v":0}]
[41,"304-NW5","centrala klimatyzacyjna","TAK","VBW","BS-3(50)-L/P",null,2010,5,null,{"$f":"I42*J42","v":0}]
[42,"304-SA-NG","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I43*J43","v":0}]
[43,"304-ST-KS1","klimatyzator ","nie","AUX","AUX-12QP/O","AUX-12QPI/I",2022,2,null,{"$f":"I44*J44","v":0}]
[44,"304-ST-KS2","klimatyzator ","nie","AUX","AUX-12QP/O","AUX-12QPI/I",2022,2,null,{"$f":"I45*J45","v":0}]
[45,"304-ST-NG","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I46*J46","v":0}]
[46,"304-T124,335","chłodnica szaf elektr.","nie","RITTAL","SK 3382100",null,2010,3,null,{"$f":"I47*J47","v":0}]
[47,"304-T224","chłodnica szaf elektr.","nie","RITTAL","SK 3382100",null,2010,3,null,{"$f":"I48*J48","v":0}]
[48,"304-T320","chłodnica szaf elektr.","nie","RITTAL","SK 3382100",null,2010,3,null,{"$f":"I49*J49","v":0}]
[49,"304-T411","chłodnica szaf elektr.","nie","RITTAL","SK 3382100",null,2010,3,null,{"$f":"I50*J50","v":0}]
[50,"311-NG1","linia grzewczo- nawiewna","nie","VBW","SPS-4/50-L-4350/350-3-1-P-T-1-(D-NW-ZW)",null,2009,2,null,{"$f":"I51*J51","v":0}]
[51,"401-KP2","klimatyzator przenośny","nie","Superhobby Market",189684,null,2010,2,null,{"$f":"I52*J52","v":0}]
[52,"401-SB","klimatyzator szafy el.","nie","RITTAL","SK3303504",null,2010,2,null,{"$f":"I53*J53","v":0}]
[53,"401-SZ1","klimatyzator szafy el.","nie","RITTAL","SK3305500",null,2015,2,null,{"$f":"I54*J54","v":0}]
[54,"401-SZ2","klimatyzator szafy el.","nie","RITTAL","SK3186930",null,2017,2,null,{"$f":"I55*J55","v":0}]
[55,"401-SZ3","klimatyzator szafy el.","nie","RITTAL","SK3186930",null,2017,2,null,{"$f":"I56*J56","v":0}]
[56,"401-SZ4","klimatyzator szafy el.","nie","RITTAL","SK3186930",null,2017,2,null,{"$f":"I57*J57","v":0}]
[57,"401-SZ5","klimatyzator szafy el.","nie","RITTAL","SK3186930",null,2017,2,null,{"$f":"I58*J58","v":0}]
[58,"401-SZ6","klimatyzator szafy el.","nie","RITTAL","SK3186930",null,2017,2,null,{"$f":"I59*J59","v":0}]
[59,"408-KA","klimatyzator Split","nie","Mitsubishi","PUHZ-P100YKA","PKA-M100KAL",2018,2,null,{"$f":"I60*J60","v":0}]
[60,"408-KB","klimatyzator Split","nie","Mitsubishi","PUHZ-P100YKA","PKA-M100KAL",2018,2,null,{"$f":"I61*J61","v":0}]
[61,"500-K1","klimatyzator Split","nie"," Fujitsu","AOYG18LFC","ASYG18LFCA",2019,3,null,{"$f":"I62*J62","v":0}]
[62,"500-K2","klimatyzator Split","nie"," Fujitsu","AOYG18LAC2","ASYG18LFCA",2019,3,null,{"$f":"I63*J63","v":0}]
[63,"500-NG10","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-P-860/250-3-1-P-J-1-(D-NW-ZW)",null,2010,2,null,{"$f":"I64*J64","v":0}]
[64,"500-NG3","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I65*J65","v":0}]
[65,"500-NG4","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I66*J66","v":0}]
[{"$f":"A66+1","v":66},"500-NG5","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I67*J67","v":0}]
[67,"500-NG6","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I68*J68","v":0}]
[68,"500-NG7","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I69*J69","v":0}]
[69,"500-NG8","Linia grzewczo-nawiewna","nie","SystemAir","VBC 160-2","kanałowy",2010,2,null,{"$f":"I70*J70","v":0}]
[70,"500-NG9","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-P-860/250-3-1-P-J-1-(D-NW-ZW)",null,2010,3,null,{"$f":"I71*J71","v":0}]
[71,"500-NW1","centrala nawiewno-wywiewna grzewcza","nie","VBW"," BS-1(50)-P",null,2010,4,null,{"$f":"I72*J72","v":0}]
[72,"500-NW2","centrala nawiewno-wywiewna grzewcza","nie","VBW"," BS-3(50)-L",null,2010,4,null,{"$f":"I73*J73","v":0}]
[73,"500-W10","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I74*J74","v":0}]
[74,"500-W11","Linia wywiewna","nie",null,"RF","łazienkowy",2010,1,null,{"$f":"I75*J75","v":0}]
[75,"500-W12","Linia wywiewna","nie","Soler$Palau","VENTUS VS-21-R-PHC","kanałowy",2010,1,null,{"$f":"I76*J76","v":0}]
[76,"500-W13","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I77*J77","v":0}]
[77,"500-W14","Linia wywiewna","nie","Soler$Palau","VENTUS VS-21-R-PHC","kanałowy",2010,1,null,{"$f":"I78*J78","v":0}]
[78,"500-W15","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I79*J79","v":0}]
[79,"500-W16","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I80*J80","v":0}]
[80,"500-W17","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I81*J81","v":0}]
[81,"500-W18","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I82*J82","v":0}]
[82,"500-W19","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I83*J83","v":0}]
[83,"500-W20","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I84*J84","v":0}]
[84,"500-W21","Linia wywiewna","nie","Soler$Palau","VENTUS VS-21-R-PHC","kanałowy",2010,1,null,{"$f":"I85*J85","v":0}]
[85,"500-W22","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I86*J86","v":0}]
[86,"500-W23","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I87*J87","v":0}]
[87,"500-W24","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I88*J88","v":0}]
[88,"500-W25","Linia wywiewna","nie",null,null,"łazienkowy",2010,1,null,{"$f":"I89*J89","v":0}]
[89,"500-W3","Linia wywiewna","nie","Soler$Palau","VENTUS VS-21-R-PHC","kanałowy",2010,1,null,{"$f":"I90*J90","v":0}]
[90,"500-W4","Linia wywiewna","nie","Soler$Palau","VENTUS VS-21-R-PHC","kanałowy",2010,1,null,{"$f":"I91*J91","v":0}]
[91,"500-W5","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I92*J92","v":0}]
[92,"500-W6","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I93*J93","v":0}]
[93,"500-W7","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I94*J94","v":0}]
[94,"500-W8","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I95*J95","v":0}]
[95,"500-W9","Linia wywiewna","nie","Venture ind.","RF","dachowy",2010,1,null,{"$f":"I96*J96","v":0}]
[96,"501-N-2LD","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-L-1700/300-3-1-P-T-1-9D-NW-ZW0",null,2010,2,null,{"$f":"I97*J97","v":0}]
[97,"501-N-2LG","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-P-2200/300-3-1-P-T-1-(D-NW-ZW)",null,2010,2,null,{"$f":"I98*J98","v":0}]
[98,"501-N-2PD","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-L-1700/300-3-1-P-T-1-(D-NW-ZW0",null,2010,2,null,{"$f":"I99*J99","v":0}]
[99,"501-N-2PG","linia grzewczo-nawiewna","nie","VBW","SPS-1/50-P-2200/300-3-1-P-T-1-(D-NW-ZW)",null,2010,2,null,{"$f":"I100*J100","v":0}]
[100,"501-NG1","linia grzewczo-nawiewna","nie","VBW","B-1(50)-P",null,2010,2,null,{"$f":"I101*J101","v":0}]
[101,"507-K4","klimatyzator Split",null,"Mitsubishi","SRC35ZSP-W","SRK35ZSP-W",2022,2,null,{"$f":"I102*J102","v":0}]
[102,"507-K5","klimatyzator Split",null,"Mitsubishi","SRC50ZSP-W","SRK50ZSP-W",2022,2,null,{"$f":"I103*J103","v":0}]
[103,"507-K1","klimatyzator Split","nie"," Fujitsu",null,"ASYG14LUCA",2015,2,null,{"$f":"I104*J104","v":0}]
[104,"507-K2","klimatyzator Split","nie"," Fujitsu","AOYG122MCE","ASYG122MCE",2015,2,null,{"$f":"I105*J105","v":0}]
[105,"507-K3","klimatyzator Split","nie","Mitsubishi","SRC 35ZSP-W","SRK35ZSP-W",2022,2,null,{"$f":"I106*J106","v":0}]
[106,"507-NW1","Centrala wentylacyjna","nie","VBW","G-GOLEM-I-01-SE-FC4/CHE/PF/WHC-R",null,2015,3,null,{"$f":"I107*J107","v":0}]
[107,"507-NW2","Centrala wentylacyjna","nie","VBW","KP-500-0-L",null,2015,3,null,{"$f":"I108*J108","v":0}]
[108,"507-NW3","Centrala wentylacyjna","nie","VBW","H-Hermes-I03-SE-FC4/CHE/WHC/CF1-R",null,2015,3,null,{"$f":"I109*J109","v":0}]
[109,"507-NW4","Centrala wentylacyjna","nie","VBW","KP-500-0-L",null,2015,3,null,{"$f":"I110*J110","v":0}]
[110,"507-W10","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I111*J111","v":0}]
[111,"507-W11","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I112*J112","v":0}]
[112,"507-W12","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I113*J113","v":0}]
[113,"507-W13","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I114*J114","v":0}]
[114,"507-W6","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I115*J115","v":0}]
[115,"507-W7","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I116*J116","v":0}]
[116,"507-W8","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I117*J117","v":0}]
[117,"507-W9","Linia wywiewna","nie","Venture industries","T 350/125","kanałowy",2015,1,null,{"$f":"I118*J118","v":0}]
[118,"600-K1","klimatyzator Split","nie","DAIKIN","RXS35G2V1B","FTXS35G2V1B",2009,2,null,{"$f":"I119*J119","v":0}]
[119,"600-K2","klimatyzator Split","TAK","PANASONIC","U 12SPEY1E8","brak danych",2010,4,null,{"$f":"I120*J120","v":0}]
[120,"600-K3","agregat wody lodowej","TAK","MTA","Cygnus tech MCCG-CY131",null,2010,5,null,{"$f":"I121*J121","v":0}]
[121,"603-K","klimatyzator Split","nie","Mitsubishi","MUZ-SF25VE","MSZ-SF25VE",2010,2,null,{"$f":"I122*J122","v":0}]
[122,"701-N1","linia grzewczo-nawiewna","nie","VBW","SWOe-2/31E-L-V-(T3+T3)-J-(FWO)",null,2010,2,null,{"$f":"I123*J123","v":0}]
[123,"701-N2","linia grzewczo-nawiewna","nie","VBW","SWOe-2/31E-L-V-(T3+T3)-J-(FWO)",null,2009,2,null,{"$f":"I124*J124","v":0}]
[124,"701-N3","Centrala wentylacyjna nawiewna","nie","Bocker Filtertechnik GMBH","wentylator rosenberg ehad 280-2                   Bocker filter AUT-KTF-A",null,2010,1,null,{"$f":"I125*J125","v":0}]
[125,"701-SZ1","klimatyzator szafy el.","nie","Rittal","SK 3332240",null,2009,3,null,{"$f":"I126*J126","v":0}]
[126,"701-SZ2","klimatyzator szafy el.","nie","Rittal","SK 3332240",null,2009,3,null,{"$f":"I127*J127","v":0}]
[127,"kont1","klimatyzator Split","nie"," Fujitsu","AOYG18LFC","ASYG18LFCA",2015,2,null,{"$f":"I128*J128","v":0}]
[128,"kont2","klimatyzator Split","nie","ASW","AS-H12B4/EFR1","LHR1DI-EU",2007,2,null,{"$f":"I129*J129","v":0}]
[129,"kont3","klimatyzator Split","nie","ASW","AS-H12B4/EFR1","LHR1DI-EU",2007,2,null,{"$f":"I130*J130","v":0}]
[{"$nulls":8},{"$f":"SUM(I2:I130)","v":276},"Razem",{"$f":"SUM(K2:K130)","v":0}]